NuDET NEUTRON

Highly efficient and gamma insensitive neutron detectors. Newly developed 6LiF/ZnS(Ag) based detectors are available in both standard and customised dimensions and available with optional HDPE moderator.

Detectors are supplied with standard 14-pin socket or with voltage dividers and MHV/ BNC connectors.

**Moderator thickness:**70 mm  
**LiF/ZnS detector:**50x100x500 mm  
**PMT:**2” with standard 14-pin  
**Mod thickness:**30 mm HDPE